**Tune-Up Tuesday #1 for August 31, 2021**

% You should be able to copy-and-paste this page into Matlab and execute it.

% Please complete each section below.

% Please include your Matlab code as well as any answers to the questions as
% MATLAB comments in the full answer that you submit on Canvas.

% (a) Copy, paste and run the Matlab code from slide 1-16 to generate a cosine signal
% at frequency 440 Hz to play it as an audio signal at a sampling rate of 8000 Hz:

**f0 = 440; % 440 Hz (A in 4th octave, or A4)**

**fs = 8000; % sampling rate in Hz (a.k.a. samples/s)**

**Ts = 1/fs; % sampling time in s**

**t = 0 : Ts : 3; % sample times from 0s to 3s**

**x = cos(2\*pi\*f0\*t);**

**sound(x, fs);**

% (b) Modify the code in (a) to change the cosine frequency to 880 Hz and run the code.
% Any difference in what you hear vs. a cosine frequency of 440 Hz?

*% Note: A note in the next higher octave is at twice the frequency. The ‘A’ note
% is 440 Hz in the fourth octave, 880 Hz in the fifth, 1760 Hz in the sixth, etc.*

**pause(4); % pause for 3s to prevent sounds from overlapping**

**f0 = 880; % change from 440 Hz (A4) to 880 Hz (A5)**

**fs = 8000; % sampling rate in samples/s**

**Ts = 1/fs; % sampling time in s**

**t = 0 : Ts : 3; % 3 seconds in duration**

**x = cos(2\*pi\*f0\*t);**

**sound(x, fs);**

**% Changing f0 from 440 Hz to 880 Hz creates a sinusoidal tone**

**% at 880 Hz that sounds like a higher frequency tone ("pitch")**

**% than the cosine at 440 Hz. They are both ‘A’ notes on the Western**

**% scale, with 440 Hz in the fourth octave and 880 Hz in the fifth.**

**% The 880 Hz tone sounds louder than the 440 Hz tone.**

% (c) Using MATLAB, plot the first 12.5 ms of the signal in the time domain using the
% **plot** command.

*% Note: The reason part (c) had asked to plot the signal over 12.5ms is so you could see the
% oscillation. Plotting the signal over 3s would have 24000 points, i.e. 3s x 8000 samples/s,
% and plotting 24000 points in a small plot window would blur together into a blue rectangle.
% This part could have been done with f0 = 440 Hz or f0 = 880 Hz.*

**f0 = 440; % change from 440 Hz (A4) to 880 Hz (A5)**

**fs = 8000; % sampling rate in samples/s**

**Ts = 1/fs; % sampling time in s**

**t = 0 : Ts : 12.5\*10^(-3);**

**x = cos(2\*pi\*f0\*t);**

**plot(t, x); % see the next page for plots for f0=440 and f0=880**

% (d) Describe your plot in (c).

**% Plot has jagged peaks and troughs. Some peaks don’t reach 1, and some
% troughs don’t reach -1, because there aren’t enough samples. Not periodic.**

**% part (c) plot with f0 = 440**

Triangular peak instead of smooth

****

Triangular trough instead of smooth

Non-smooth peaks that don’t reach 1

**% part (c) plot with f0 = 880 Hz**

****

Non-smooth troughs that don’t reach -1