| RTOS_MSPM0 1.1 ECE445M starter code

WifiSettings.h
1 // WifiSettings.h
2 // Dung Nguyen
3 // Wally Guzman
4
5 // Launchpad or TM4C123
6 #define LAUNCHPAD 1
7
8 // Baudrate for UART connection to ESP8266
9 //#define BAUDRATE 74880 // The ESP first boots with 74880 baud and then switches
10 #define BAUDRATE 115200
11
12 // Return values
13 #define NORESPONSE (-1)
14 #define BADVALUE (-1)
15 #define SUCCESS 1
16 #define FAILURE 0
17
18 enum Menu_Status {RX=0, TX, CONNECTED};
19
20 // Station or soft access point mode
21 // 0 means regular station, 1 means act as soft AP
22 #define SOFTAP 0
23
24 // Access Point Parameters
25 // #define SSID_NAME "YourAP"
26 // #define PASSKEY "YourPassword"
27
28 #define SSID_NAME "utexas-iot"
29 #define PASSKEY ""
30
31 /* To get the password for the "utexas-iot" network:
32
33 From your PC/laptop:
34
35 Go to https://network.utexas.edu
36 Log in with your UT EID (via UTLogin)
37 Click the "Register Wireless Device" button
38 Enter your device's MAC address and a description, and click the "Register" button
39 Make note of the WPA2 key generated (will be unique for each device you register)
40
41 On your IoT device:
42
43 Select utexas-iot from the available wireless networks
44 Enter the WPA2 key provided to you in step 5 above
45
46 */