| RTOS_MSPM0 1.1 ECE445M starter code

Functions
UART2.h File Reference
UART

Initialize UART2, no transmit, interrupt on receive timeout. More...

Go to the source code of this file.

## Functions
void | UART2_Init (void)
| Initialize UART1. More...
char | UART2_InChar (void)
| get data from FIFO1 More...

## Detailed Description

Initialize UART2, no transmit, interrupt on receive timeout.

UART2 initialization. 2000 bps baud, 1 start, 8 data bits, 1 stop, no parity.

Version
  ECE319K v1.0

Author
  your name

Copyright
  lab 8 solution, do not post,

Warning
  AS-IS

Note
  For more information see http://users.ece.utexas.edu/~valvano/

Date
  October 29, 2023

  UART pins on the MSPM0G3507
  Pin | Description
  --- | ---
  PA22 | UART2 Rx from other microcontroller PA8 Tx
  J14 | Connect SW1 to PA9 (not PB23)