MSPM0
Recovery Action 3. Force BSL with physical Reset:

    Press-and-hold the BSL_Invoke button (S2, near LED) while pressing and releasing the Reset button.
    The device should go to BSL and stay in Active mode for ~10secs.
    Attempt to program immediately after releasing reset.

