(kicad_pcb (version 20221018) (generator pcbnew)
  (general
    (thickness 1.6)
  )
  (paper "A4")
  (title_block
    (title "ECE 319K Baseline Project")
    (date "2023-10-30")
    (rev "v1.0.0")
    (company "The University of Texas at Austin")
  )
  (layers
    (0 "F.Cu" signal)
    (31 "B.Cu" signal)
    (32 "B.Adhes" user "B.Adhesive")
    (33 "F.Adhes" user "F.Adhesive")
    (34 "B.Paste" user)
    (35 "F.Paste" user)
    (36 "B.SilkS" user "B.Silkscreen")
    (37 "F.SilkS" user "F.Silkscreen")
    (38 "B.Mask" user)
    (39 "F.Mask" user)
    (40 "Dwgs.User" user "User.Drawings")
    (41 "Cmts.User" user "User.Comments")
    (42 "Eco1.User" user "User.Eco1")
    (43 "Eco2.User" user "User.Eco2")
    (44 "Edge.Cuts" user)
    (45 "Margin" user)
    (46 "B.CrtYd" user "B.Courtyard")
    (47 "F.CrtYd" user "F.Courtyard")
    (48 "B.Fab" user)
    (49 "F.Fab" user)
    (50 "User.1" user)
    (51 "User.2" user)
    (52 "User.3" user)
    (53 "User.4" user)
    (54 "User.5" user)
    (55 "User.6" user)
    (56 "User.7" user)
    (57 "User.8" user)
    (58 "User.9" user)
  )
  (setup
    (stackup
      (layer "F.SilkS" (type "Top Silk Screen"))
      (layer "F.Paste" (type "Top Solder Paste"))
      (layer "F.Mask" (type "Top Solder Mask") (thickness 0.01))
      (layer "F.Cu" (type "copper") (thickness 0.035))
      (layer "dielectric 1" (type "core") (thickness 1.51) (material "FR4") (epsilon_r 4.5) (loss_tangent 0.02))
      (layer "B.Cu" (type "copper") (thickness 0.035))
      (layer "B.Mask" (type "Bottom Solder Mask") (thickness 0.01))
      (layer "B.Paste" (type "Bottom Solder Paste"))
      (layer "B.SilkS" (type "Bottom Silk Screen"))
      (copper_finish "None")
      (dielectric_constraints no)
    )
    (pad_to_mask_clearance 0)
    (pcbplotparams
      (layerselection 0x00010fc_ffffffff)
      (plot_on_all_layers_selection 0x0000000_00000000)
      (disableapertmacros false)
      (usegerberextensions true)
      (usegerberattributes false)
      (usegerberadvancedattributes false)
      (creategerberjobfile false)
      (dashed_line_dash_ratio 12.000000)
      (dashed_line_gap_ratio 3.000000)
      (svgprecision 4)
      (plotframeref false)
      (viasonmask false)
      (mode 1)
      (useauxorigin false)
      (hpglpennumber 1)
      (hpglpenspeed 20)
      (hpglpendiameter 15.000000)
      (dxfpolygonmode true)
      (dxfimperialunits true)
      (dxfusepcbnewfont true)
      (psnegative false)
      (psa4output false)
      (plotreference true)
      (plotvalue false)
      (plotinvisibletext false)
      (sketchpadsonfab false)
      (subtractmaskfromsilk true)
      (outputformat 1)
      (mirror false)
      (drillshape 0)
      (scaleselection 1)
      (outputdirectory "plots/")
    )
  )
  (net 0 "")
  (net 1 "GND")
  (net 2 "+3V3")
  (net 3 "PB9")
  (net 4 "PB15")
  (net 5 "PB8")
  (net 6 "PB7")
  (net 7 "PB6")
  (net 8 "PA13")
  (net 9 "+5V")
  (net 10 "unconnected-(C1-Pad1)")
  (net 11 "unconnected-(C1-Pad2)")
  (net 12 "unconnected-(C2-Pad1)")
  (net 13 "unconnected-(C2-Pad2)")
  (net 14 "unconnected-(C3-Pad1)")
  (net 15 "PA25")
  (net 16 "unconnected-(C3-Pad2)")
  (net 17 "PA8")
  (net 18 "PA26")
  (net 19 "PB24")
  (net 20 "PA27")
  (net 21 "PB2")
  (net 22 "PB3")
  (net 23 "unconnected-(U2-~{TARGETRST}-PadJ2_5)")
  (net 24 "PB12")
  (net 25 "PB17")
  (net 26 "PB0")
  (net 27 "PB16")
  (net 28 "PB19")
  (net 29 "PA22")
  (net 30 "PB18")
  (net 31 "PA18")
  (net 32 "PA24")
  (net 33 "PA17")
  (net 34 "PA16")
  (net 35 "PA15")
  (net 36 "PB4")
  (net 37 "PB1")
  (net 38 "PA28")
  (net 39 "PA31")
  (net 40 "PB20")
  (net 41 "PB13")
  (net 42 "PA10")
  (net 43 "unconnected-(D1-K-Pad1)")
  (net 44 "unconnected-(D1-A-Pad2)")
  (net 45 "unconnected-(D2-K-Pad1)")
  (net 46 "PB23")
  (net 47 "unconnected-(D2-A-Pad2)")
  (net 48 "PA11")
  (net 49 "PA12")
  (net 50 "unconnected-(U4-Pin3-Pad3)")
  (net 51 "unconnected-(U4-Pin4-Pad4)")
  (net 52 "unconnected-(U4-Pin5-Pad5)")
  (net 53 "unconnected-(RV1-PadMP)")
  (net 54 "unconnected-(H1-Hole-Pad1)")
  (net 55 "unconnected-(H2-Hole-Pad1)")
  (net 56 "unconnected-(H3-Hole-Pad1)")
  (net 57 "unconnected-(H4-Hole-Pad1)")
  (net 58 "unconnected-(D3-K-Pad1)")
  (net 59 "unconnected-(D3-A-Pad2)")
  (net 60 "unconnected-(J1-ring-PadR)")
  (net 61 "unconnected-(J1-sleeve-PadS)")
  (net 62 "unconnected-(J1-tip-PadT)")
  (net 63 "unconnected-(J2-Pad1)")
  (net 64 "unconnected-(J2-Pad2)")
  (net 65 "unconnected-(J4-A-Pad1)")
  (net 66 "unconnected-(J4-B-Pad2)")
  (net 67 "unconnected-(J7-A-Pad1)")
  (net 68 "unconnected-(J7-B-Pad2)")
  (net 69 "unconnected-(JP1-A-Pad1)")
  (net 70 "unconnected-(JP1-B-Pad3)")
  (net 71 "unconnected-(R1-Pad1)")
  (net 72 "unconnected-(R1-Pad2)")
  (net 73 "unconnected-(R2-Pad1)")
  (net 74 "unconnected-(R2-Pad2)")
  (net 75 "unconnected-(R3-Pad1)")
  (net 76 "unconnected-(R3-Pad2)")
  (net 77 "unconnected-(R4-Pad1)")
  (net 78 "unconnected-(R4-Pad2)")
  (net 79 "unconnected-(R5-Pad1)")
  (net 80 "unconnected-(R5-Pad2)")
  (net 81 "unconnected-(R6-Pad1)")
  (net 82 "unconnected-(R6-Pad2)")
  (net 83 "unconnected-(R7-Pad1)")
  (net 84 "unconnected-(R7-Pad2)")
  (net 85 "unconnected-(R8-Pad1)")
  (net 86 "unconnected-(R8-Pad2)")
  (net 87 "unconnected-(R9-Pad1)")
  (net 88 "unconnected-(R9-Pad2)")
  (net 89 "unconnected-(R10-Pad1)")
  (net 90 "unconnected-(R10-Pad2)")
  (net 91 "unconnected-(R11-Pad1)")
  (net 92 "unconnected-(R11-Pad2)")
  (net 93 "unconnected-(R12-Pad1)")
  (net 94 "unconnected-(R12-Pad2)")
  (net 95 "unconnected-(R13-Pad1)")
  (net 96 "unconnected-(R13-Pad2)")
  (net 97 "unconnected-(R14-Pad1)")
  (net 98 "unconnected-(R14-Pad2)")
  (net 99 "unconnected-(R15-Pad1)")
  (net 100 "unconnected-(R15-Pad2)")
  (net 101 "unconnected-(R16-Pad1)")
  (net 102 "unconnected-(R16-Pad2)")
  (net 103 "unconnected-(R17-Pad1)")
  (net 104 "unconnected-(R17-Pad2)")
  (net 105 "unconnected-(RV1-Pad1)")
  (net 106 "unconnected-(RV1-Pad2)")
  (net 107 "unconnected-(SW1-Pad1)")
  (net 108 "unconnected-(SW1-Pad2)")
  (net 109 "unconnected-(SW2-Pad1)")
  (net 110 "unconnected-(SW2-Pad2)")
  (net 111 "unconnected-(SW3-Pad1)")
  (net 112 "unconnected-(SW3-Pad2)")
  (net 113 "unconnected-(SW4-Pad1)")
  (net 114 "unconnected-(SW4-Pad2)")
  (net 115 "unconnected-(U3-CD-Pad1)")
  (net 116 "unconnected-(U3-FC2-Pad2)")
  (net 117 "unconnected-(U3-FC1-Pad3)")
  (net 118 "unconnected-(U3-VIN-Pad4)")
  (net 119 "unconnected-(U3-VO1-Pad5)")
  (net 120 "unconnected-(U3-Vcc-Pad6)")
  (net 121 "unconnected-(U3-GND-Pad7)")
  (net 122 "unconnected-(U3-VO2-Pad8)")
  (net 123 "unconnected-(RV1-Pad3)")
  (footprint "ECE319K:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal" (layer "F.Cu")
    (at 90.17 25.4)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "Starter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small US symbol")
    (property "ki_keywords" "r resistor")
    (attr through_hole)
    (fp_text reference "R11" (at 1.905 -1.92) (layer "F.SilkS"))
    (fp_text value "12k" (at 5.08 -1.905) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 91 "unconnected-(R11-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 92 "unconnected-(R11-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "ECE319K:Testpoint_1x02_P2.54mm" (layer "F.Cu")
    (at 86.36 134.62 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (property "Sheetfile" "Starter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Testpoint")
    (property "ki_keywords" "Testpoint")
    (attr through_hole)
    (fp_text reference "J4" (at 0 -2.33 90) (layer "F.Fab"))
    (fp_text value "Pot" (at 1.905 1.275) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 1.27 180) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 65 "unconnected-(J4-A-Pad1)") (pinfunction "A") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 66 "unconnected-(J4-B-Pad2)") (pinfunction "B") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "ECE319K:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal" (layer "F.Cu")
    (at 74.93 33.02)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "Starter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small US symbol")
    (property "ki_keywords" "r resistor")
    (attr through_hole)
    (fp_text reference "R4" (at 1.27 -1.92) (layer "F.SilkS"))
    (fp_text value "1.5k" (at 5.08 -1.905) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 77 "unconnected-(R4-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 78 "unconnected-(R4-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "ECE319K:PinHeader_1x03_P2.54mm_Vertical" (layer "F.Cu")
    (at 141.62 30.48 90)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (property "Sheetfile" "Starter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Header, 3-pin")
    (property "ki_keywords" "Header")
    (attr through_hole)
    (fp_text reference "J3" (at 0 -2.33 90) (layer "F.SilkS") hide)
    (fp_text value "UART1" (at -2.54 2.525) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "A") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 17 "PA8") (pinfunction "B") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 29 "PA22") (pinfunction "C") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "LOGO" (layer "F.Cu")
    (at 180.34 71.12)
    (attr board_only exclude_from_pos_files exclude_from_bom)
    (fp_text reference "G***" (at 0 0) (layer "F.SilkS") hide)
    (fp_text value "LOGO" (at 0.75 0) (layer "F.SilkS") hide)
  )
  (footprint "ECE319K:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal" (layer "F.Cu")
    (at 72.39 27.94)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "Starter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small US symbol")
    (property "ki_keywords" "r resistor")
    (attr through_hole)
    (fp_text reference "R6" (at 1.27 -1.905) (layer "F.SilkS"))
    (fp_text value "1.5k" (at 5.08 -1.905) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 81 "unconnected-(R6-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 82 "unconnected-(R6-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "ECE319K:DIP-8_W7.62mm_LongPads" (layer "F.Cu")
    (at 35.56 88.9 -90)
    (descr "8-lead though-hole mounted DIP package, row spacing 7.62 mm (300 mils), LongPads")
    (tags "THT DIP DIL PDIP 2.54mm 7.62mm 300mil LongPads")
    (property "Cost" "N/A")
    (property "Distributor" "N/A")
    (property "LCSC Part #" "")
    (property "Manufacturer" "Motorola")
    (property "P/N" "MC34119P")
    (property "Sheetfile" "Starter.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U3" (at 3.81 -2.33 90) (layer "F.SilkS"))
    (fp_text value "MCP34119P" (at 3.81 9.95 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 3.81 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0 270) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 115 "unconnected-(U3-CD-Pad1)") (pinfunction "CD") (pintype "input"))
    (pad "2" thru_hole oval (at 0 2.54 270) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 116 "unconnected-(U3-FC2-Pad2)") (pinfunction "FC2") (pintype "input"))
    (pad "3" thru_hole oval (at 0 5.08 270) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 117 "unconnected-(U3-FC1-Pad3)") (pinfunction "FC1") (pintype "input"))
    (pad "4" thru_hole oval (at 0 7.62 270) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 118 "unconnected-(U3-VIN-Pad4)") (pinfunction "VIN") (pintype "input"))
    (pad "5" thru_hole oval (at 7.62 7.62 270) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 119 "unconnected-(U3-VO1-Pad5)") (pinfunction "VO1") (pintype "output"))
    (pad "6" thru_hole oval (at 7.62 5.08 270) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 120 "unconnected-(U3-Vcc-Pad6)") (pinfunction "Vcc") (pintype "power_in"))
    (pad "7" thru_hole oval (at 7.62 2.54 270) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 121 "unconnected-(U3-GND-Pad7)") (pinfunction "GND") (pintype "power_in"))
    (pad "8" thru_hole oval (at 7.62 0 270) (size 2.4 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 122 "unconnected-(U3-VO2-Pad8)") (pinfunction "VO2") (pintype "output"))
    (model "${KICAD6_3DMODEL_DIR}/Package_DIP.3dshapes/DIP-8_W7.62mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "ECE319K:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal" (layer "F.Cu")
    (at 40.64 92.71 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "Starter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small US symbol")
    (property "ki_keywords" "r resistor")
    (attr through_hole)
    (fp_text reference "R17" (at 1.905 -2.54 90) (layer "F.SilkS"))
    (fp_text value "10k" (at 5.08 -2.54 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 103 "unconnected-(R17-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 90) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 104 "unconnected-(R17-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "ECE319K:SW_PUSH_6mm" (layer "F.Cu")
    (at 36.68 121.92)
    (descr "https://www.omron.com/ecb/products/pdf/en-b3f.pdf")
    (tags "tact sw push 6mm")
    (property "Sheetfile" "Starter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Push button switch, generic, two pins")
    (property "ki_keywords" "switch normally-open pushbutton push-button")
    (attr through_hole)
    (fp_text reference "SW2" (at 3.325 -1.905) (layer "F.SilkS"))
    (fp_text value "LEFT" (at 3.75 6.7) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 3.25 2.25) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 2 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 109 "unconnected-(SW2-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "1" thru_hole circle (at 6.5 0 90) (size 2 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 109 "unconnected-(SW2-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 4.5 90) (size 2 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 110 "unconnected-(SW2-Pad2)") (pinfunction "2") (pintype "passive"))
    (pad "2" thru_hole circle (at 6.5 4.5 90) (size 2 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 110 "unconnected-(SW2-Pad2)") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_THT.3dshapes/SW_PUSH_6mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "ECE319K:SW_PUSH_6mm" (layer "F.Cu")
    (at 34.85 109.51)
    (descr "https://www.omron.com/ecb/products/pdf/en-b3f.pdf")
    (tags "tact sw push 6mm")
    (property "Sheetfile" "Starter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Push button switch, generic, two pins")
    (property "ki_keywords" "switch normally-open pushbutton push-button")
    (attr through_hole)
    (fp_text reference "SW1" (at 3.25 -2) (layer "F.SilkS"))
    (fp_text value "UP" (at 3.75 6.7) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 3.25 2.25) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 2 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 107 "unconnected-(SW1-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "1" thru_hole circle (at 6.5 0 90) (size 2 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 107 "unconnected-(SW1-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 4.5 90) (size 2 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 108 "unconnected-(SW1-Pad2)") (pinfunction "2") (pintype "passive"))
    (pad "2" thru_hole circle (at 6.5 4.5 90) (size 2 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 108 "unconnected-(SW1-Pad2)") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_THT.3dshapes/SW_PUSH_6mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "ECE319K:PTA2043pot" (layer "F.Cu")
    (at 171.565 140.49)
    (descr "Bourns single-gang slide potentiometer, 20.0mm travel, https://www.bourns.com/docs/Product-Datasheets/pta.pdf")
    (tags "Bourns single-gang slide potentiometer 20.0mm")
    (property "Sheetfile" "Starter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Potentiometer, US symbol")
    (property "ki_keywords" "resistor variable")
    (attr through_hole)
    (fp_text reference "RV1" (at 16.5 -4) (layer "F.SilkS"))
    (fp_text value "PTA2043" (at 16.5 7.5) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 16.5 1.75) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.75 1.75) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 105 "unconnected-(RV1-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 3.5) (size 1.75 1.75) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 106 "unconnected-(RV1-Pad2)") (pinfunction "2") (pintype "passive"))
    (pad "3" thru_hole circle (at 33 0) (size 1.75 1.75) (drill 1.2) (layers "*.Cu" "*.Mask")
      (net 123 "unconnected-(RV1-Pad3)") (pinfunction "3") (pintype "passive"))
    (pad "MP" thru_hole circle (at 3.9 5.95) (size 2.7 2.7) (drill 1.7) (layers "*.Cu" "*.Mask")
      (net 53 "unconnected-(RV1-PadMP)") (pinfunction "MP") (pintype "free"))
    (pad "MP" thru_hole circle (at 5.1 -2.45) (size 2.7 2.7) (drill 1.7) (layers "*.Cu" "*.Mask")
      (net 53 "unconnected-(RV1-PadMP)") (pinfunction "MP") (pintype "free"))
    (pad "MP" thru_hole circle (at 27.9 -2.45) (size 2.7 2.7) (drill 1.7) (layers "*.Cu" "*.Mask")
      (net 53 "unconnected-(RV1-PadMP)") (pinfunction "MP") (pintype "free"))
    (pad "MP" thru_hole circle (at 29.1 5.95) (size 2.7 2.7) (drill 1.7) (layers "*.Cu" "*.Mask")
      (net 53 "unconnected-(RV1-PadMP)") (pinfunction "MP") (pintype "free"))
    (model "${KICAD6_3DMODEL_DIR}/Potentiometer_THT.3dshapes/Potentiometer_Bourns_PTA2043_Single_Slide.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "ECE319K:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal" (layer "F.Cu")
    (at 124.46 25.4)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "Starter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small US symbol")
    (property "ki_keywords" "r resistor")
    (attr through_hole)
    (fp_text reference "R10" (at 1.89 -1.905) (layer "F.SilkS"))
    (fp_text value "12k" (at 5.08 -1.905) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 89 "unconnected-(R10-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 90 "unconnected-(R10-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "ECE319K:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal" (layer "F.Cu")
    (at 170.18 59.69 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "Starter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small US symbol")
    (property "ki_keywords" "r resistor")
    (attr through_hole)
    (fp_text reference "R1" (at 3.81 -1.92 90) (layer "F.SilkS"))
    (fp_text value "470" (at 3.81 1.92 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 71 "unconnected-(R1-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 90) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 72 "unconnected-(R1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "ECE319K:Testpoint_1x02_P2.54mm" (layer "F.Cu")
    (at 66.67 33.02 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (property "Sheetfile" "Starter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Testpoint")
    (property "ki_keywords" "Testpoint")
    (attr through_hole)
    (fp_text reference "J7" (at 0 -2.33 90) (layer "F.Fab"))
    (fp_text value "DACOUT" (at 1.905 1.275) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 1.27 180) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 67 "unconnected-(J7-A-Pad1)") (pinfunction "A") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 68 "unconnected-(J7-B-Pad2)") (pinfunction "B") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "ECE319K:Testpoint_1x02_P2.54mm" (layer "F.Cu")
    (at 142.24 132.08 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (property "Sheetfile" "Starter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Testpoint")
    (property "ki_keywords" "Testpoint")
    (attr through_hole)
    (fp_text reference "TP1" (at 0 -3.81) (layer "F.Fab"))
    (fp_text value "3.3V" (at 1.905 1.905) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 1.27) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "+3V3") (pinfunction "A") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 2 "+3V3") (pinfunction "B") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "ECE319K:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal" (layer "F.Cu")
    (at 102.87 25.4)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "Starter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small US symbol")
    (property "ki_keywords" "r resistor")
    (attr through_hole)
    (fp_text reference "R8" (at 1.905 -1.905) (layer "F.SilkS"))
    (fp_text value "1.5k" (at 5.08 -1.905) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 85 "unconnected-(R8-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 86 "unconnected-(R8-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "ECE319K:C_Axial_200mil" (layer "F.Cu")
    (at 38.1 68.58 -90)
    (descr "C, Axial series, Axial, Horizontal, pin pitch=15mm, , length*diameter=5.1*3.1mm^2, http://www.vishay.com/docs/45231/arseries.pdf")
    (tags "C Axial series Axial Horizontal pin pitch 15mm  length 5.1mm diameter 3.1mm")
    (property "Sheetfile" "Starter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Unpolarized capacitor")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C3" (at 4.445 -2.54 90) (layer "F.SilkS"))
    (fp_text value "0.1uF" (at 3.175 2.67 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at -0.635 3.175 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 14 "unconnected-(C3-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 5.08 0 270) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 16 "unconnected-(C3-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/C_Axial_L5.1mm_D3.1mm_P15.00mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "ECE319K:MountingHole_4_40" (layer "F.Cu")
    (at 161.29 41.91)
    (descr "Mounting Hole 0.125in")
    (tags "mounting hole 0.125in 4_40")
    (property "Sheetfile" "Starter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Drill hole for 4-40 screw")
    (attr exclude_from_pos_files)
    (fp_text reference "H2" (at -3.175 -2.54) (layer "F.Fab"))
    (fp_text value "~" (at 0 4) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 4.318 4.318) (drill 3.175) (layers "*.Cu" "*.Mask")
      (net 55 "unconnected-(H2-Hole-Pad1)") (pinfunction "Hole") (pintype "power_in"))
  )
  (footprint "ECE319K:MountingHole_4_40" (layer "F.Cu")
    (at 161.29 123.19)
    (descr "Mounting Hole 0.125in")
    (tags "mounting hole 0.125in 4_40")
    (property "Sheetfile" "Starter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Drill hole for 4-40 screw")
    (attr exclude_from_pos_files)
    (fp_text reference "H4" (at 0 -4) (layer "F.Fab"))
    (fp_text value "~" (at 0 4) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 4.318 4.318) (drill 3.175) (layers "*.Cu" "*.Mask")
      (net 57 "unconnected-(H4-Hole-Pad1)") (pinfunction "Hole") (pintype "power_in"))
  )
  (footprint "ECE319K:MountingHole_4_40" (layer "F.Cu")
    (at 54.61 41.91)
    (descr "Mounting Hole 0.125in")
    (tags "mounting hole 0.125in 4_40")
    (property "Sheetfile" "Starter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Drill hole for 4-40 screw")
    (attr exclude_from_pos_files)
    (fp_text reference "H1" (at 2.54 -2.54) (layer "F.Fab"))
    (fp_text value "~" (at 0 4) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 4.318 4.318) (drill 3.175) (layers "*.Cu" "*.Mask")
      (net 54 "unconnected-(H1-Hole-Pad1)") (pinfunction "Hole") (pintype "power_in"))
  )
  (footprint "ECE319K:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal" (layer "F.Cu")
    (at 29.21 119.38 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "Starter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small US symbol")
    (property "ki_keywords" "r resistor")
    (attr through_hole)
    (fp_text reference "R12" (at 3.81 1.905) (layer "F.SilkS"))
    (fp_text value "10k" (at 3.81 -1.905) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 93 "unconnected-(R12-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 180) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 94 "unconnected-(R12-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "ECE319K:hiletgo_st7735r" (layer "F.Cu")
    (at 255.27 59.69)
    (property "Cost" "9.95")
    (property "Distributor" "Amazon")
    (property "LCSC Part #" "")
    (property "Manufacturer" "HiLetGo")
    (property "P/N" "https://www.amazon.com/s?k=hiletgo+ST7735R")
    (property "Sheetfile" "Starter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "http://hiletgo.com/ProductDetail/2157911.html")
    (attr through_hole)
    (fp_text reference "U4" (at -12.7 24.765) (layer "F.SilkS"))
    (fp_text value "HiLetGo_ST7735R" (at 24.13 19.05 90) (layer "F.Fab"))
    (fp_text user "Up" (at -1.27 -17.78 unlocked) (layer "F.SilkS"))
    (fp_text user "1" (at -20.32 -25.4 unlocked) (layer "F.SilkS"))
    (fp_text user "(0,0)" (at -13.97 -17.78 unlocked) (layer "F.SilkS"))
    (fp_text user "(127,159)" (at 7.62 20.32 unlocked) (layer "F.SilkS"))
    (pad "" np_thru_hole circle (at 19.685 20.32 90) (size 3.81 3.81) (drill 3.175) (layers "F&B.Cu" "*.Mask"))
    (pad "1" thru_hole rect (at -19.05 -24.13 90) (size 1.778 1.778) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in") (solder_mask_margin 0.102))
    (pad "2" thru_hole circle (at -16.51 -24.13 90) (size 1.778 1.778) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 2 "+3V3") (pinfunction "VCC") (pintype "power_in") (solder_mask_margin 0.102))
    (pad "3" thru_hole circle (at -13.97 -24.13 90) (size 1.778 1.778) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 50 "unconnected-(U4-Pin3-Pad3)") (pinfunction "Pin3") (pintype "free") (solder_mask_margin 0.102))
    (pad "4" thru_hole circle (at -11.43 -24.13 90) (size 1.778 1.778) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 51 "unconnected-(U4-Pin4-Pad4)") (pinfunction "Pin4") (pintype "free") (solder_mask_margin 0.102))
    (pad "5" thru_hole circle (at -8.89 -24.13 90) (size 1.778 1.778) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 52 "unconnected-(U4-Pin5-Pad5)") (pinfunction "Pin5") (pintype "free") (solder_mask_margin 0.102))
    (pad "6" thru_hole circle (at -6.35 -24.13 90) (size 1.778 1.778) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 4 "PB15") (pinfunction "RESET") (pintype "input") (solder_mask_margin 0.102))
    (pad "7" thru_hole circle (at -3.81 -24.13 90) (size 1.778 1.778) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 8 "PA13") (pinfunction "TFTDC") (pintype "input") (solder_mask_margin 0.102))
    (pad "8" thru_hole circle (at -1.27 -24.13 90) (size 1.778 1.778) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 5 "PB8") (pinfunction "TFTMOSI") (pintype "input") (solder_mask_margin 0.102))
    (pad "9" thru_hole circle (at 1.27 -24.13 90) (size 1.778 1.778) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 3 "PB9") (pinfunction "TFTSCK") (pintype "input") (solder_mask_margin 0.102))
    (pad "10" thru_hole circle (at 3.81 -24.13 90) (size 1.778 1.778) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 7 "PB6") (pinfunction "TFT_CS") (pintype "input") (solder_mask_margin 0.102))
    (pad "11" thru_hole circle (at 6.35 -24.13 90) (size 1.778 1.778) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 3 "PB9") (pinfunction "SDCSCK") (pintype "input") (solder_mask_margin 0.102))
    (pad "12" thru_hole circle (at 8.89 -24.13 90) (size 1.778 1.778) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 6 "PB7") (pinfunction "SDC_MISO") (pintype "output") (solder_mask_margin 0.102))
    (pad "13" thru_hole circle (at 11.43 -24.13 90) (size 1.778 1.778) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 5 "PB8") (pinfunction "SDC_MOSI") (pintype "input") (solder_mask_margin 0.102))
    (pad "14" thru_hole circle (at 13.97 -24.13 90) (size 1.778 1.778) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 49 "PA12") (pinfunction "SDC_CS") (pintype "input") (solder_mask_margin 0.102))
    (pad "15" thru_hole circle (at 16.51 -24.13 90) (size 1.778 1.778) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 2 "+3V3") (pinfunction "LED+") (pintype "power_in") (solder_mask_margin 0.102))
    (pad "16" thru_hole circle (at 19.05 -24.13 90) (size 1.778 1.778) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "LED-") (pintype "power_in") (solder_mask_margin 0.102))
    (model "${KIPRJMOD}/models/adafruit_st7735r.stp"
      (offset (xyz 29 -17.5 2.5))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD7_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x08_P2.54mm_Vertical.wrl"
      (offset (xyz -25.25 9 2.5))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
  )
  (footprint "ECE319K:MountingHole_4_40" (layer "F.Cu")
    (at 54.61 123.19)
    (descr "Mounting Hole 0.125in")
    (tags "mounting hole 0.125in 4_40")
    (property "Sheetfile" "Starter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Drill hole for 4-40 screw")
    (attr exclude_from_pos_files)
    (fp_text reference "H3" (at 0 -4) (layer "F.Fab"))
    (fp_text value "~" (at 0 4) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 4.318 4.318) (drill 3.175) (layers "*.Cu" "*.Mask")
      (net 56 "unconnected-(H3-Hole-Pad1)") (pinfunction "Hole") (pintype "power_in"))
  )
  (footprint "ECE319K:CP_Radial_Tantal200mil" (layer "F.Cu")
    (at 15.24 81.28)
    (descr "CP, Radial_Tantal series, Radial, pin pitch=200mil, , diameter=6.0mm, Tantal Electrolytic Capacitor")
    (tags "CP Radial_Tantal series Radial pin pitch 200mil  diameter 6.0mm Tantal Electrolytic Capacitor")
    (property "Sheetfile" "Starter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Polarized capacitor, US symbol")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C2" (at 0.595 -3.81) (layer "F.SilkS"))
    (fp_text value "4.7uF" (at 5.675 -3.81) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 12 "unconnected-(C2-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 5.08 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 13 "unconnected-(C2-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_Tantal_D6.0mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "ECE319K:Testpoint_1x02_P2.54mm" (layer "F.Cu")
    (at 150.49 132.08 90)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (property "Sheetfile" "Starter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Testpoint")
    (property "ki_keywords" "Testpoint")
    (attr through_hole)
    (fp_text reference "J6" (at 0 -2.33 90) (layer "F.Fab"))
    (fp_text value "GND" (at 1.905 1.91) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 1.27 180) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "A") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54 90) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "B") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "ECE319K:LED_D5.0mm" (layer "F.Cu")
    (at 187.96 43.18)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (property "Sheetfile" "Starter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Light emitting diode")
    (property "ki_keywords" "LED diode")
    (attr through_hole)
    (fp_text reference "D3" (at 1.27 -3.96) (layer "F.SilkS"))
    (fp_text value "LED" (at 1.27 3.96) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 58 "unconnected-(D3-K-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 59 "unconnected-(D3-A-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "ECE319K:CP_Radial_Tantal200mil" (layer "F.Cu")
    (at 15.24 93.98)
    (descr "CP, Radial_Tantal series, Radial, pin pitch=200mil, , diameter=6.0mm, Tantal Electrolytic Capacitor")
    (tags "CP Radial_Tantal series Radial pin pitch 200mil  diameter 6.0mm Tantal Electrolytic Capacitor")
    (property "Sheetfile" "Starter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Polarized capacitor, US symbol")
    (property "ki_keywords" "cap capacitor")
    (attr through_hole)
    (fp_text reference "C1" (at 0 -3.81) (layer "F.SilkS"))
    (fp_text value "1uF" (at 5.08 -3.81) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 2.5 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 10 "unconnected-(C1-Pad1)") (pintype "passive"))
    (pad "2" thru_hole circle (at 5.08 0) (size 1.6 1.6) (drill 0.8) (layers "*.Cu" "*.Mask")
      (net 11 "unconnected-(C1-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Capacitor_THT.3dshapes/CP_Radial_Tantal_D6.0mm_P5.00mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "ECE319K:SW_PUSH_6mm" (layer "F.Cu")
    (at 34.85 134.91)
    (descr "https://www.omron.com/ecb/products/pdf/en-b3f.pdf")
    (tags "tact sw push 6mm")
    (property "Sheetfile" "Starter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Push button switch, generic, two pins")
    (property "ki_keywords" "switch normally-open pushbutton push-button")
    (attr through_hole)
    (fp_text reference "SW4" (at 3.25 -2) (layer "F.SilkS"))
    (fp_text value "RGHT" (at 3.75 6.7) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 3.25 2.25) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 2 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 113 "unconnected-(SW4-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "1" thru_hole circle (at 6.5 0 90) (size 2 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 113 "unconnected-(SW4-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 4.5 90) (size 2 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 114 "unconnected-(SW4-Pad2)") (pinfunction "2") (pintype "passive"))
    (pad "2" thru_hole circle (at 6.5 4.5 90) (size 2 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 114 "unconnected-(SW4-Pad2)") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_THT.3dshapes/SW_PUSH_6mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "ECE319K:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal" (layer "F.Cu")
    (at 180.34 54.61 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "Starter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small US symbol")
    (property "ki_keywords" "r resistor")
    (attr through_hole)
    (fp_text reference "R3" (at 3.81 -1.92 90) (layer "F.SilkS"))
    (fp_text value "470" (at 3.81 1.92 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 75 "unconnected-(R3-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 90) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 76 "unconnected-(R3-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "ECE319K:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal" (layer "F.Cu")
    (at 29.21 124.46 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "Starter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small US symbol")
    (property "ki_keywords" "r resistor")
    (attr through_hole)
    (fp_text reference "R13" (at 3.81 1.905) (layer "F.SilkS"))
    (fp_text value "10k" (at 3.81 -1.905) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 95 "unconnected-(R13-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 180) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 96 "unconnected-(R13-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "ECE319K:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal" (layer "F.Cu")
    (at 175.26 49.53 90)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "Starter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small US symbol")
    (property "ki_keywords" "r resistor")
    (attr through_hole)
    (fp_text reference "R2" (at 3.81 -1.92 90) (layer "F.SilkS"))
    (fp_text value "470" (at 3.81 1.92 90) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0 90) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 73 "unconnected-(R2-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 90) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 74 "unconnected-(R2-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "ECE319K:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal" (layer "F.Cu")
    (at 31.75 81.28)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "Starter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small US symbol")
    (property "ki_keywords" "r resistor")
    (attr through_hole)
    (fp_text reference "R16" (at 0.635 -1.92) (layer "F.SilkS"))
    (fp_text value "20k" (at 3.81 -1.905) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 101 "unconnected-(R16-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 102 "unconnected-(R16-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "ECE319K:Jack_3.5mm_CUI_SJ1-3523N_Horizontal" (layer "F.Cu")
    (at 33.1 53.34 -90)
    (descr "TRS 3.5mm, horizontal, through-hole, https://www.cuidevices.com/product/resource/pdf/sj1-352xn.pdf")
    (tags "TRS audio jack stereo horizontal")
    (property "Sheetfile" "Starter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Speaker")
    (property "ki_keywords" "headphone sound")
    (attr through_hole exclude_from_pos_files)
    (fp_text reference "J1" (at 2.62 -3.175) (layer "F.SilkS"))
    (fp_text value "AudioJack" (at 7.065 -1.905) (layer "F.Fab"))
    (fp_text user "PCB edge" (at 0 3.65 -90 unlocked) (layer "Dwgs.User"))
    (fp_text user "${REFERENCE}" (at 0 -1.5 90) (layer "F.Fab"))
    (pad "" np_thru_hole circle (at -5 0 270) (size 1.2 1.2) (drill 1.2) (layers "*.Cu"))
    (pad "" np_thru_hole circle (at -5 2.5 270) (size 1.2 1.2) (drill 1.2) (layers "*.Cu"))
    (pad "" np_thru_hole circle (at 0 -5 270) (size 1.2 1.2) (drill 1.2) (layers "*.Cu"))
    (pad "" np_thru_hole circle (at 5 0 270) (size 1.2 1.2) (drill 1.2) (layers "*.Cu"))
    (pad "" np_thru_hole circle (at 5 2.5 270) (size 1.2 1.2) (drill 1.2) (layers "*.Cu"))
    (pad "R" thru_hole oval (at -5 -5 270) (size 1.27 2.286) (drill oval 0.635 1.524) (layers "*.Cu" "*.Mask")
      (net 60 "unconnected-(J1-ring-PadR)") (pinfunction "ring") (pintype "input"))
    (pad "S" thru_hole oval (at 0 0 270) (size 2.286 1.27) (drill oval 1.524 0.635) (layers "*.Cu" "*.Mask")
      (net 61 "unconnected-(J1-sleeve-PadS)") (pinfunction "sleeve") (pintype "input"))
    (pad "T" thru_hole oval (at 5 -5 90) (size 1.27 2.286) (drill oval 0.635 1.524) (layers "*.Cu" "*.Mask")
      (net 62 "unconnected-(J1-tip-PadT)") (pinfunction "tip") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_Audio.3dshapes/Jack_3.5mm_CUI_SJ1-3523N_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "ECE319K:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal" (layer "F.Cu")
    (at 34.29 104.14 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "Starter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small US symbol")
    (property "ki_keywords" "r resistor")
    (attr through_hole)
    (fp_text reference "R15" (at 3.81 1.905) (layer "F.SilkS"))
    (fp_text value "10k" (at 3.81 -1.905) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 99 "unconnected-(R15-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 180) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 100 "unconnected-(R15-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "ECE319K:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal" (layer "F.Cu")
    (at 100.33 35.56)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "Starter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small US symbol")
    (property "ki_keywords" "r resistor")
    (attr through_hole)
    (fp_text reference "R9" (at 1.905 -1.92) (layer "F.SilkS"))
    (fp_text value "12k" (at 5.08 -1.905) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 87 "unconnected-(R9-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 88 "unconnected-(R9-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "ECE319K:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal" (layer "F.Cu")
    (at 27.94 111.76 180)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "Starter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small US symbol")
    (property "ki_keywords" "r resistor")
    (attr through_hole)
    (fp_text reference "R14" (at 3.81 1.905) (layer "F.SilkS"))
    (fp_text value "10k" (at 3.81 -1.905) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 180) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 97 "unconnected-(R14-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0 180) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 98 "unconnected-(R14-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "ECE319K:SW_PUSH_6mm" (layer "F.Cu")
    (at 55.17 134.91)
    (descr "https://www.omron.com/ecb/products/pdf/en-b3f.pdf")
    (tags "tact sw push 6mm")
    (property "Sheetfile" "Starter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Push button switch, generic, two pins")
    (property "ki_keywords" "switch normally-open pushbutton push-button")
    (attr through_hole)
    (fp_text reference "SW3" (at 3.25 -2) (layer "F.SilkS"))
    (fp_text value "DOWN" (at 3.75 6.7) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 3.25 2.25) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0 90) (size 2 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 111 "unconnected-(SW3-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "1" thru_hole circle (at 6.5 0 90) (size 2 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 111 "unconnected-(SW3-Pad1)") (pinfunction "1") (pintype "passive"))
    (pad "2" thru_hole circle (at 0 4.5 90) (size 2 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 112 "unconnected-(SW3-Pad2)") (pinfunction "2") (pintype "passive"))
    (pad "2" thru_hole circle (at 6.5 4.5 90) (size 2 2) (drill 1.1) (layers "*.Cu" "*.Mask")
      (net 112 "unconnected-(SW3-Pad2)") (pinfunction "2") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Button_Switch_THT.3dshapes/SW_PUSH_6mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "ECE319K:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal" (layer "F.Cu")
    (at 85.09 33.02)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "Starter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small US symbol")
    (property "ki_keywords" "r resistor")
    (attr through_hole)
    (fp_text reference "R5" (at 1.27 -1.905) (layer "F.SilkS"))
    (fp_text value "1.5k" (at 5.08 -1.905) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 79 "unconnected-(R5-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 80 "unconnected-(R5-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "ECE319K:R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal" (layer "F.Cu")
    (at 102.87 30.48)
    (descr "Resistor, Axial_DIN0204 series, Axial, Horizontal, pin pitch=7.62mm, 0.167W, length*diameter=3.6*1.6mm^2, http://cdn-reichelt.de/documents/datenblatt/B400/1_4W%23YAG.pdf")
    (tags "Resistor Axial_DIN0204 series Axial Horizontal pin pitch 7.62mm 0.167W length 3.6mm diameter 1.6mm")
    (property "Sheetfile" "Starter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Resistor, small US symbol")
    (property "ki_keywords" "r resistor")
    (attr through_hole)
    (fp_text reference "R7" (at 1.27 -1.905) (layer "F.SilkS"))
    (fp_text value "1.5k" (at 5.08 -1.905) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 3.81 0) (layer "F.Fab"))
    (pad "1" thru_hole circle (at 0 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 83 "unconnected-(R7-Pad1)") (pintype "passive"))
    (pad "2" thru_hole oval (at 7.62 0) (size 1.4 1.4) (drill 0.7) (layers "*.Cu" "*.Mask")
      (net 84 "unconnected-(R7-Pad2)") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Resistor_THT.3dshapes/R_Axial_DIN0204_L3.6mm_D1.6mm_P7.62mm_Horizontal.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "ECE319K:PinHeader_1x02_P2.54mm_Vertical" (layer "F.Cu")
    (at 43.18 99.06)
    (descr "Through hole straight pin header, 1x02, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x02 2.54mm single row")
    (property "Sheetfile" "Starter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Speaker")
    (property "ki_keywords" "speaker sound")
    (attr through_hole)
    (fp_text reference "J2" (at 0 -2.33) (layer "F.SilkS"))
    (fp_text value "Speaker" (at 0.635 5.08) (layer "F.SilkS"))
    (fp_text user "${REFERENCE}" (at 0 1.27 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 63 "unconnected-(J2-Pad1)") (pinfunction "1") (pintype "input"))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 64 "unconnected-(J2-Pad2)") (pinfunction "2") (pintype "input"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x02_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "ECE319K:LED_D5.0mm" (layer "F.Cu")
    (at 160.02 27.94)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (property "Sheetfile" "Starter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Light emitting diode")
    (property "ki_keywords" "LED diode")
    (attr through_hole)
    (fp_text reference "D1" (at 1.27 -3.96) (layer "F.SilkS"))
    (fp_text value "LED" (at 1.27 3.96) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 43 "unconnected-(D1-K-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 44 "unconnected-(D1-A-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "ECE319K:PinHeader_1x03_P2.54mm_Vertical" (layer "F.Cu")
    (at 45.72 60.96)
    (descr "Through hole straight pin header, 1x03, 2.54mm pitch, single row")
    (tags "Through hole pin header THT 1x03 2.54mm single row")
    (property "Sheetfile" "Starter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Jumper, 3-pole, both open")
    (property "ki_keywords" "Jumper SPDT")
    (attr through_hole)
    (fp_text reference "JP1" (at 0 -2.33) (layer "F.SilkS"))
    (fp_text value "TExaS" (at 0 7.41) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 0 2.54 90) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 69 "unconnected-(JP1-A-Pad1)") (pinfunction "A") (pintype "passive"))
    (pad "2" thru_hole oval (at 0 2.54) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 40 "PB20") (pinfunction "C") (pintype "passive"))
    (pad "3" thru_hole oval (at 0 5.08) (size 1.7 1.7) (drill 1) (layers "*.Cu" "*.Mask")
      (net 70 "unconnected-(JP1-B-Pad3)") (pinfunction "B") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x03_P2.54mm_Vertical.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "ECE319K:LED_D5.0mm" (layer "F.Cu")
    (at 177.8 30.48)
    (descr "LED, diameter 5.0mm, 2 pins, http://cdn-reichelt.de/documents/datenblatt/A500/LL-504BC2E-009.pdf")
    (tags "LED diameter 5.0mm 2 pins")
    (property "Sheetfile" "Starter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "Light emitting diode")
    (property "ki_keywords" "LED diode")
    (attr through_hole)
    (fp_text reference "D2" (at 1.27 -3.96) (layer "F.SilkS"))
    (fp_text value "LED" (at 1.27 3.96) (layer "F.Fab"))
    (fp_text user "${REFERENCE}" (at 1.25 0) (layer "F.Fab"))
    (pad "1" thru_hole rect (at 0 0) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 45 "unconnected-(D2-K-Pad1)") (pinfunction "K") (pintype "passive"))
    (pad "2" thru_hole circle (at 2.54 0) (size 1.8 1.8) (drill 0.9) (layers "*.Cu" "*.Mask")
      (net 47 "unconnected-(D2-A-Pad2)") (pinfunction "A") (pintype "passive"))
    (model "${KICAD6_3DMODEL_DIR}/LED_THT.3dshapes/LED_D5.0mm.wrl"
      (offset (xyz 0 0 0))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (footprint "ECE319K:adafruit_st7735r" (layer "F.Cu")
    (at 246.38 121.92)
    (property "Cost" "19.95")
    (property "Distributor" "Mouser")
    (property "LCSC Part #" "")
    (property "Manufacturer" "Adafruit")
    (property "P/N" "358")
    (property "Sheetfile" "Starter.kicad_sch")
    (property "Sheetname" "")
    (attr through_hole)
    (fp_text reference "U1" (at -15.24 31.75) (layer "F.SilkS"))
    (fp_text value "Adafruit ST7735R" (at 19.03 21.84 90) (layer "F.Fab"))
    (fp_text user "(0,0)" (at -13.97 -17.78 unlocked) (layer "F.SilkS"))
    (fp_text user "1" (at -12.7 24.13 unlocked) (layer "F.SilkS"))
    (fp_text user "(127,159)" (at 7.62 20.32 unlocked) (layer "F.SilkS"))
    (pad "" np_thru_hole circle (at -14.605 -25.4 90) (size 2.2 2.2) (drill 2.2) (layers "*.Cu" "*.Mask"))
    (pad "" np_thru_hole circle (at -14.605 25.4 90) (size 2.2 2.2) (drill 2.2) (layers "F&B.Cu" "*.Mask"))
    (pad "" np_thru_hole circle (at 14.605 -25.4 90) (size 2.2 2.2) (drill 2.2) (layers "F&B.Cu" "*.Mask"))
    (pad "" np_thru_hole circle (at 14.605 25.4 90) (size 2.2 2.2) (drill 2.2) (layers "F&B.Cu" "*.Mask"))
    (pad "1" thru_hole rect (at -11.43 25.4 90) (size 1.778 1.778) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_in") (solder_mask_margin 0.102))
    (pad "2" thru_hole circle (at -8.89 25.4 90) (size 1.778 1.778) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 2 "+3V3") (pinfunction "VCC") (pintype "power_in") (solder_mask_margin 0.102))
    (pad "3" thru_hole circle (at -6.35 25.4 90) (size 1.778 1.778) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 4 "PB15") (pinfunction "RESET") (pintype "input") (solder_mask_margin 0.102))
    (pad "4" thru_hole circle (at -3.81 25.4 90) (size 1.778 1.778) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 8 "PA13") (pinfunction "D/C") (pintype "input") (solder_mask_margin 0.102))
    (pad "5" thru_hole circle (at -1.27 25.4 90) (size 1.778 1.778) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 49 "PA12") (pinfunction "CARD_CS") (pintype "input") (solder_mask_margin 0.102))
    (pad "6" thru_hole circle (at 1.27 25.4 90) (size 1.778 1.778) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 7 "PB6") (pinfunction "TFT_CS") (pintype "input") (solder_mask_margin 0.102))
    (pad "7" thru_hole circle (at 3.81 25.4 90) (size 1.778 1.778) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 5 "PB8") (pinfunction "MOSI") (pintype "input") (solder_mask_margin 0.102))
    (pad "8" thru_hole circle (at 6.35 25.4 90) (size 1.778 1.778) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 3 "PB9") (pinfunction "SCK") (pintype "input") (solder_mask_margin 0.102))
    (pad "9" thru_hole circle (at 8.89 25.4 90) (size 1.778 1.778) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 6 "PB7") (pinfunction "MISO") (pintype "output") (solder_mask_margin 0.102))
    (pad "10" thru_hole circle (at 11.43 25.4 90) (size 1.778 1.778) (drill 1.016) (layers "*.Cu" "*.Mask")
      (net 2 "+3V3") (pinfunction "LITE") (pintype "power_in") (solder_mask_margin 0.102))
    (model "${KIPRJMOD}/models/adafruit_st7735r.stp"
      (offset (xyz 29 -17.5 2.5))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
    (model "${KICAD7_3DMODEL_DIR}/Connector_PinHeader_2.54mm.3dshapes/PinHeader_1x08_P2.54mm_Vertical.wrl"
      (offset (xyz -25.25 9 2.5))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 180 0))
    )
  )
  (footprint "ECE319K:ti_LP_MSPM0G3507" (layer "B.Cu")
    (at 106.68 81.28 -90)
    (property "Cost" "22.60")
    (property "Distributor" "Mouser")
    (property "LCSC Part #" "")
    (property "Manufacturer" "Texas Instruments")
    (property "P/N" "LP-MSPM0G3507")
    (property "Sheetfile" "Starter.kicad_sch")
    (property "Sheetname" "")
    (property "ki_description" "LaunchPad")
    (attr through_hole)
    (fp_text reference "U2" (at -22.86 45.72 -270) (layer "B.SilkS"))
    (fp_text value "LP-MSPM0G3507" (at -17.78 -45.72 -270) (layer "B.Fab"))
    (fp_text user "Reset" (at 15.24 51.435 -270 unlocked) (layer "B.SilkS"))
    (fp_text user "USB" (at -21.59 51.435 -270 unlocked) (layer "B.SilkS"))
    (fp_text user "S1" (at -26.67 7.62 -270 unlocked) (layer "B.SilkS"))
    (fp_text user "S2" (at 25.4 7.62 -270 unlocked) (layer "B.SilkS"))
    (dimension (type aligned) (layer "Cmts.User")
      (pts (xy 127 93.98) (xy 157.48 93.98))
      (height 2.54)
      (gr_text "1.200" (at 142.24 95.42) (layer "Cmts.User"))
      (format (prefix "") (suffix "") (units 0) (units_format 0) (precision 3))
      (style (thickness 0.1) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
    )
    (dimension (type aligned) (layer "Cmts.User")
      (pts (xy 104.14 88.9) (xy 53.34 88.9))
      (height -5.08)
      (gr_text "2.000" (at 78.74 92.88) (layer "Cmts.User"))
      (format (prefix "") (suffix "") (units 0) (units_format 0) (precision 3))
      (style (thickness 0.1) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
    )
    (dimension (type aligned) (layer "Cmts.User")
      (pts (xy 73.66 53.34) (xy 73.66 109.22))
      (height 2.54)
      (gr_text "2.200" (at 70.02 81.28 90) (layer "Cmts.User"))
      (format (prefix "") (suffix "") (units 0) (units_format 0) (precision 3))
      (style (thickness 0.1) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
    )
    (dimension (type aligned) (layer "Cmts.User")
      (pts (xy 53.34 68.58) (xy 157.48 68.58))
      (height 5.08)
      (gr_text "4.100" (at 105.41 72.56) (layer "Cmts.User"))
      (format (prefix "") (suffix "") (units 0) (units_format 0) (precision 3))
      (style (thickness 0.1) (arrow_length 1.27) (text_position_mode 0) (extension_height 0.58642) (extension_offset 0.5) keep_text_aligned)
    )
    (pad "J1_1" thru_hole rect (at -22.86 2.54 270) (size 1.52 1.52) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 2 "+3V3") (pinfunction "+3.3V") (pintype "power_out") (solder_mask_margin 0.102))
    (pad "J1_2" thru_hole circle (at -22.86 0 270) (size 1.52 1.52) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 15 "PA25") (pinfunction "PA25") (pintype "bidirectional") (solder_mask_margin 0.102))
    (pad "J1_3" thru_hole circle (at -22.86 -2.54 270) (size 1.52 1.52) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 46 "PB23") (pinfunction "PA9/PB23") (pintype "bidirectional") (solder_mask_margin 0.102))
    (pad "J1_4" thru_hole circle (at -22.86 -5.08 270) (size 1.52 1.52) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 17 "PA8") (pinfunction "PA8") (pintype "bidirectional") (solder_mask_margin 0.102))
    (pad "J1_5" thru_hole circle (at -22.86 -7.62 270) (size 1.52 1.52) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 18 "PA26") (pinfunction "PA26") (pintype "bidirectional") (solder_mask_margin 0.102))
    (pad "J1_6" thru_hole circle (at -22.86 -10.16 270) (size 1.52 1.52) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 19 "PB24") (pinfunction "PB24") (pintype "bidirectional") (solder_mask_margin 0.102))
    (pad "J1_7" thru_hole circle (at -22.86 -12.7 270) (size 1.52 1.52) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 3 "PB9") (pinfunction "PB9") (pintype "bidirectional") (solder_mask_margin 0.102))
    (pad "J1_8" thru_hole circle (at -22.86 -15.24 270) (size 1.52 1.52) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 20 "PA27") (pinfunction "PA27") (pintype "bidirectional") (solder_mask_margin 0.102))
    (pad "J1_9" thru_hole circle (at -22.86 -17.78 270) (size 1.52 1.52) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 21 "PB2") (pinfunction "PB2") (pintype "bidirectional") (solder_mask_margin 0.102))
    (pad "J1_10" thru_hole circle (at -22.86 -20.32 270) (size 1.52 1.52) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 22 "PB3") (pinfunction "PB3") (pintype "bidirectional") (solder_mask_margin 0.102))
    (pad "J2_1" thru_hole circle (at 22.86 2.54 270) (size 1.52 1.52) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_out") (solder_mask_margin 0.102))
    (pad "J2_2" thru_hole circle (at 22.86 0 270) (size 1.52 1.52) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 24 "PB12") (pinfunction "PB12") (pintype "bidirectional") (solder_mask_margin 0.102))
    (pad "J2_3" thru_hole circle (at 22.86 -2.54 270) (size 1.52 1.52) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 25 "PB17") (pinfunction "PB17") (pintype "bidirectional") (solder_mask_margin 0.102))
    (pad "J2_4" thru_hole circle (at 22.86 -5.08 270) (size 1.52 1.52) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 4 "PB15") (pinfunction "PB15") (pintype "bidirectional") (solder_mask_margin 0.102))
    (pad "J2_5" thru_hole circle (at 22.86 -7.62 270) (size 1.52 1.52) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 23 "unconnected-(U2-~{TARGETRST}-PadJ2_5)") (pinfunction "~{TARGETRST}") (pintype "input") (solder_mask_margin 0.102))
    (pad "J2_6" thru_hole circle (at 22.86 -10.16 270) (size 1.52 1.52) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 5 "PB8") (pinfunction "PB8") (pintype "bidirectional") (solder_mask_margin 0.102))
    (pad "J2_7" thru_hole circle (at 22.86 -12.7 270) (size 1.52 1.52) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 6 "PB7") (pinfunction "PB7") (pintype "bidirectional") (solder_mask_margin 0.102))
    (pad "J2_8" thru_hole circle (at 22.86 -15.24 270) (size 1.52 1.52) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 7 "PB6") (pinfunction "PB6") (pintype "bidirectional") (solder_mask_margin 0.102))
    (pad "J2_9" thru_hole circle (at 22.86 -17.78 270) (size 1.52 1.52) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 26 "PB0") (pinfunction "PB0") (pintype "bidirectional") (solder_mask_margin 0.102))
    (pad "J2_10" thru_hole circle (at 22.86 -20.32 270) (size 1.52 1.52) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 27 "PB16") (pinfunction "PB16") (pintype "bidirectional") (solder_mask_margin 0.102))
    (pad "J3_1" thru_hole circle (at -20.32 2.54 270) (size 1.52 1.52) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 9 "+5V") (pinfunction "+VBUS") (pintype "power_out") (solder_mask_margin 0.102))
    (pad "J3_2" thru_hole circle (at -20.32 0 270) (size 1.52 1.52) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 1 "GND") (pinfunction "GND") (pintype "power_out") (solder_mask_margin 0.102))
    (pad "J3_3" thru_hole circle (at -20.32 -2.54 270) (size 1.52 1.52) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 28 "PB19") (pinfunction "PB19") (pintype "bidirectional") (solder_mask_margin 0.102))
    (pad "J3_4" thru_hole circle (at -20.32 -5.08 270) (size 1.52 1.52) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 29 "PA22") (pinfunction "PA22") (pintype "bidirectional") (solder_mask_margin 0.102))
    (pad "J3_5" thru_hole circle (at -20.32 -7.62 270) (size 1.52 1.52) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 30 "PB18") (pinfunction "PB18") (pintype "bidirectional") (solder_mask_margin 0.102))
    (pad "J3_6" thru_hole circle (at -20.32 -10.16 270) (size 1.52 1.52) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 31 "PA18") (pinfunction "PA18") (pintype "bidirectional") (solder_mask_margin 0.102))
    (pad "J3_7" thru_hole circle (at -20.32 -12.7 270) (size 1.52 1.52) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 32 "PA24") (pinfunction "PA24") (pintype "bidirectional") (solder_mask_margin 0.102))
    (pad "J3_8" thru_hole circle (at -20.32 -15.24 270) (size 1.52 1.52) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 33 "PA17") (pinfunction "PA17") (pintype "bidirectional") (solder_mask_margin 0.102))
    (pad "J3_9" thru_hole circle (at -20.32 -17.78 270) (size 1.52 1.52) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 34 "PA16") (pinfunction "PA16") (pintype "bidirectional") (solder_mask_margin 0.102))
    (pad "J3_10" thru_hole circle (at -20.32 -20.32 270) (size 1.52 1.52) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 35 "PA15") (pinfunction "PA15") (pintype "bidirectional") (solder_mask_margin 0.102))
    (pad "J4_1" thru_hole circle (at 20.32 2.54 270) (size 1.52 1.52) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 36 "PB4") (pinfunction "PB4") (pintype "bidirectional") (solder_mask_margin 0.102))
    (pad "J4_2" thru_hole circle (at 20.32 0 270) (size 1.52 1.52) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 37 "PB1") (pinfunction "PB1") (pintype "bidirectional") (solder_mask_margin 0.102))
    (pad "J4_3" thru_hole circle (at 20.32 -2.54 270) (size 1.52 1.52) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 38 "PA28") (pinfunction "PA28") (pintype "bidirectional") (solder_mask_margin 0.102))
    (pad "J4_4" thru_hole circle (at 20.32 -5.08 270) (size 1.52 1.52) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 39 "PA31") (pinfunction "PA31") (pintype "bidirectional") (solder_mask_margin 0.102))
    (pad "J4_5" thru_hole circle (at 20.32 -7.62 270) (size 1.52 1.52) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 40 "PB20") (pinfunction "PB20") (pintype "bidirectional") (solder_mask_margin 0.102))
    (pad "J4_6" thru_hole circle (at 20.32 -10.16 270) (size 1.52 1.52) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 41 "PB13") (pinfunction "PB13") (pintype "bidirectional") (solder_mask_margin 0.102))
    (pad "J4_7" thru_hole circle (at 20.32 -12.7 270) (size 1.52 1.52) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 42 "PA10") (pinfunction "PA10") (pintype "bidirectional") (solder_mask_margin 0.102))
    (pad "J4_8" thru_hole circle (at 20.32 -15.24 270) (size 1.52 1.52) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 48 "PA11") (pinfunction "PA11") (pintype "bidirectional") (solder_mask_margin 0.102))
    (pad "J4_9" thru_hole circle (at 20.32 -17.78 270) (size 1.52 1.52) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 49 "PA12") (pinfunction "PA12") (pintype "bidirectional") (solder_mask_margin 0.102))
    (pad "J4_10" thru_hole circle (at 20.32 -20.32 270) (size 1.52 1.52) (drill 0.89) (layers "*.Cu" "*.Mask")
      (net 8 "PA13") (pinfunction "PA13") (pintype "bidirectional") (solder_mask_margin 0.102))
    (model "${KIPRJMOD}/models/ti_EKTM4C123GXL.step"
      (offset (xyz 0 0 8))
      (scale (xyz 1 1 1))
      (rotate (xyz 0 0 0))
    )
  )
  (gr_rect (start 50.8 38.1) (end 165.1 127)
    (fill none) (layer "Edge.Cuts"))
  (gr_text "Your names\n" (at 185.42 109.22) (layer "B.SilkS"))
  (gr_text "U1Rx" (at 142.875 27.94) (layer "F.SilkS"))
  (gr_text "GND" (at 140.335 27.94) (layer "F.SilkS"))
  (gr_text "Your names" (at 182.88 114.3) (layer "F.SilkS"))
  (gr_text "POT" (at 41.275 66.675) (layer "F.SilkS"))
  (gr_text "U1Tx" (at 146.05 27.94) (layer "F.SilkS"))
  (gr_text "ECE319K PCB camp \nFall 2023" (at 172.72 93.98) (layer "F.SilkS"))
  (gr_text "DACOUT" (at 39.37 60.96) (layer "F.SilkS"))
  (gr_text "TExaS" (at 40.64 64.135) (layer "F.SilkS"))
)
