ADCSWTrigger

Readme This is a C language project that demonstrates the analog to digital converter (ADC). main1 samples one channel, the accelerometer Y from PA22. main2 demonstrates using the sequencer sampling two channels, the accelerometer X from PB19 and the accelerometer Z from PB18. main interfaces the MKII joystick sampling two channels, the joystick X from PA25 and the joystick Y from PA18. This example also inputs from the joystick switch. Derived from Texas Instrument code adc12_single_conversion_vref_internal_LP_MSPM0G3507_nortos_ticlang adc12_single_conversion_LP_MSPM0G3507_nortos_ticlang

Hardware Required MSPM0G3507 LaunchPad™ Development Kit (LP-MSPM0G3507) Educational BoosterPack MKII (BOOSTXL-EDUMKII) Pin assignments Digital Input: PA26 is MKII joystick Select button Analog Input: PA25 is MKII joystick horizontal (X) PA25_ADC0.2 Analog Input: PA18 is MKII joystick vertical (Y) PA18_ADC1.3 Analog Input: MKII is accelerometer X PB19__ADC1.6 Analog Input: MKII is accelerometer Y PA22__ADC0.7 Analog Input: MKII is accelerometer Z PB18__ADC1.5 Output: PA0 is red LED1, index 0 in IOMUX PINCM table Output: PB22 is blue LED2, index 49 in IOMUX PINCM table Output: PB26 is red LED2, index 56 in IOMUX PINCM table Output: PB27 is green LED2, index 57 in IOMUX PINCM table Input: PA18 is S2 positive logic switch, index 39 in IOMUX PINCM table Input: PB21 is S3 negative logic switch, index 48 in IOMUX PINCM table LaunchPad Jumpers Remove J16 J17 J18: Disconnects light sensor from the microcontroller PA22 PA27 PA26 J4: Connects PA0 to red LED J5: Connects PB22 to blue LED2 J6: Connects PB26 to red LED2 J7: Connects PB27 to green LED2

Simplified BSD License (FreeBSD License) Copyright © 2023, Jonathan Valvano, All rights reserved.
Redistribution and use in source and binary forms, with or without modification, are permitted provided that the following conditions are met:

1. Redistributions of source code must retain the above copyright notice, this list of conditions and the following disclaimer.
2. Redistributions in binary form must reproduce the above copyright notice, this list of conditions and the following disclaimer in the documentation and/or other materials provided with the distribution.

THIS SOFTWARE IS PROVIDED BY THE COPYRIGHT HOLDERS AND CONTRIBUTORS "AS IS" AND ANY EXPRESS OR IMPLIED WARRANTIES, INCLUDING, BUT NOT LIMITED TO, THE IMPLIED WARRANTIES OF MERCHANTABILITY AND FITNESS FOR A PARTICULAR PURPOSE ARE DISCLAIMED. IN NO EVENT SHALL THE COPYRIGHT OWNER OR CONTRIBUTORS BE LIABLE FOR ANY DIRECT, INDIRECT, INCIDENTAL, SPECIAL, EXEMPLARY, OR CONSEQUENTIAL DAMAGES (INCLUDING, BUT NOT LIMITED TO, PROCUREMENT OF SUBSTITUTE GOODS OR SERVICES; LOSS OF USE, DATA, OR PROFITS; OR BUSINESS INTERRUPTION) HOWEVER CAUSED AND ON ANY THEORY OF LIABILITY, WHETHER IN CONTRACT, STRICT LIABILITY, OR TORT (INCLUDING NEGLIGENCE OR OTHERWISE) ARISING IN ANY WAY OUT OF THE USE OF THIS SOFTWARE, EVEN IF ADVISED OF THE POSSIBILITY OF SUCH DAMAGE.
The views and conclusions contained in the software and documentation are those of the authors and should not be interpreted as representing official policies, either expressed or implied, of the FreeBSD Project.

For more information, see http://users.ece.utexas.edu/~valvano/.